Suppl Fig. 1: Receiver operating characteristics (ROC) and areas under the curves (AUC).for optimum FASILA cutoff