

Figure S1: Optical images with crossed polarizers of two drops of 5.5wt% CNCs in water (A) and 5wt% CNCs in 10 mM NaCl (B). Some birefringence is always visible along the rim due to the alignment of CNCs upon drying. Scale bar 250 μm.